Loading 7 real STL groups…
X right · Y rear · Z up

## Computed optical layout

Each sensor from vertical 86°
Included optical-axis angle 172°
Ideal spherical union 78.81%
Two MID‑360 units cannot cover a full sphere: the official −7°…+52° vertical band leaves 21.19% ideal blind area. Hardware occlusion is additional.

## Assembly · click to isolate

394 × 338 × 360 mm 71 objects 83 solids 8 fabrication STLs

## Downloads

FreeCAD editable FCStd Assembly visual STL STEP neutral B‑rep Package CAD + parts + report BOM selected components Verification checks + SHA‑256

## Design basis

Official Livox MID‑360 STEP; Seeed reComputer J4012; Waveshare 5.5″ AMOLED; CSBattery LFP24V10; Noctua NF‑A6x25; Vicor DCM3623T36G13C2T00. See engineering report.